LabVIEW Software: LabVIEW 2.1.10.0

TULV_API.dll:
File Version: 2.1.5.0
Product Version: 2.1.10.0

TUCam.dll:
File Version: 2.0.8.0
Product Version: 2.0.7.0

Applicable Cameras:
1. Dhyana 401D, Dhyana 201D, Dhyana 95 V2, Dhyana 400BSI V3
2. Other models are compatible but have not been systematically tested. Some features may not be optimal or may have potential issues. Users should contact us if they encounter problems.

Update Notes:
1. This version supports all functions of the optimized Dhyana 400BSI V3, Dhyana 95 V2, Dhyana 401D, and Dhyana 201D standard cameras. Other cameras have not been tested.
2. The plugin is available only in X64 and supports LabVIEW 2016, with backward compatibility.
3. For untested cameras, if no new requirements are provided, older plugins will continue to be offered. New compatibility requirements will be considered in this version.
4. Added features: frame capture from memory, image storage, and stacking functionality. The GetFrameIndexDemo.vi retrieves memory data for a specific ID, displaying all-zero data when exceeding memory capacity. The MultiDataDemo.vi supports stack settings, allowing the capture and saving of multiple images as stacked TIFF and RAW files.